For 1990-2009 cars

### Removal Procedure

1. Remove the front seat back cushion cover. Refer to Front Seat Back Cushion Cover Replacement.
2. Remove the front seat backrest adjustment lever.

• | Remove the clamp.

• | Remove the lever in direction of the arrow.

3. Remove the cover for the front seat backrest adjustment lever (1).

Release the 4 clips.

### Installation Procedure

1. Install the cover for the front seat backrest adjustment lever.

Install the 4 clips.

2. Install the fastening clamp, release lever.
3. Install the front seat backrest adjustment lever.

• | Install the clamp, release lever.

• | Insert the lever.

4. Install the front seat back cushion cover. Refer to Front Seat Back Cushion Cover Replacement.