For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
ZAT08 XE | ZAR48 XE ZAT48 XR | ZAT08 XE | ZAR48 XE ZAT48 XR
Front Wheel Opening (P) | 655.0 mm | 665.0 mm | 25.78 in | 26.18 in
Rear Wheel Opening (R) | 659.0 mm | 670.0 mm | 25.94 in | 26.37 in

• | The front wheel opening height P (P) is measured from the bottom lip of the wheel opening to the ground, measured at the center line of the front wheel.

• | The rear wheel opening height R (R) is measured from the bottom lip of the wheel opening to the ground, measured at the center line of the rear wheel.

All measurements are taken with a full tank of gas.

All measurements have a tolerance of ±15 mm (0.60 in).