For 1990-2009 cars

### Removal Procedure

1. Remove the upholstery covering for front seat backs. Refer to Front Seat Back Cushion Cover Replacement .
2. Remove the front seat backrest adjustment lever.

2.1. | Remove the clamp.

2.2. | Remove the lever in direction of arrow.

3. Remove the cover for front seat backrest adjustment lever (1).

Unclip the 4 clips.

4. Remove the release cable for front seat backrest.

4.1. | Remove the cable tie (arrow).

4.2. | Release the upper release cable (1).

4.3. | Unclip the 4 clips from the upper release cable bracket.

4.4. | Remove the 2 retaining rings (2), lower the release cable.

4.5. | Unclip the 2 lower guide clamps (3).

5. Release and remove the lower release cable.

### Installation Procedure

1. Install the release cable for front seat backrest.

1.1. | Install the lower release cable.

1.2. | Install the 2 retaining rings, lower release cable.

1.3. | Clip in the 2 lower guide clamps.

1.4. | Clip in the 4 clips in the upper release cable bracket.

1.5. | Install the upper release cable.

1.6. | Install the cable ties.

2. Install the cover for the front seat backrest adjustment lever.

Clip in the 4 clips.

3. Install the fastening clamp, release the lever.
4. Install the front seat backrest adjustment lever.

4.1. | Install the clamp, release the lever.

4.2. | Insert the lever.

5. Install the upholstery covering for front seat backrest. Refer to Front Seat Back Cushion Cover Replacement .