For 1990-2009 cars

### Removal Procedure

1. Remove the rear storage compartment in the front floor console.

• | Remove the storage compartment in the direction of the arrow.

• | Disconnect the wiring harness plug (1).

2. Remove the rear seat audio control from the storage compartment.

Release the 3 clips (2).

### Installation Procedure

1. Install the rear seat audio control into the storage compartment.

Install in the 6 clips.

2. Install the rear storage compartment into the front floor console.

Connect the wiring harness plug.