For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Assist Handle Bolts | 2.8 N·m | 23 lb in
Cargo Net Bracket Bolt | 20 N·m | 15 lb ft
Center Pillar Deflection Sheave Bolt | 30 N·m | 22 lb ft
Front Side Door Trim Panel Bolts | 1.5 N·m | 13 lb in
Quarter Trim Panel Bolts - Lower | 35 N·m | 26 lb ft
Quarter Trim Panel Bolts - Upper | 2.5 N·m | 22 lb in
Rear Compartment Side Trim Bolts | 2.5 N·m | 22 lb in
Rear Seat Backrest Bolt | 40 N·m | 30 lb ft
Rear Seat Backrest Bolts - Front and Rear | 20 N·m | 15 lb ft
Rear Seat Backrest Front Screws/Bolts with the Belt Buckle | 35 N·m | 26 lb ft
Rear Seat Backrest Front Belt Buckle Bolts | 20 N·m | 15 lb ft
Rear Seat Backrest to Seat Belt Buckle Bolts | 20 N·m | 15 lb ft
Rear Side Door Trim Panel Screws | 1.5 N·m | 13 lb in
Rear Quarter Trim Panel Bolts | 2.5 N·m | 22 lb in
Seat Belt Bolt | 35 N·m | 26 lb ft
Seat Belt Buckle Bolts | 35 N·m | 26 lb ft
Seat Belt Bolts - Center Pillar | 35 N·m | 26 lb ft
Seat Belt Rear Quarter Bolts | 35 N·m | 26 lb ft
Seat Belt Striker - Lower | 35 N·m | 26 lb ft
Seat Belt to Center Pillar Bolt | 35 N·m | 26 lb ft
Seat Belt to Front Seat Bolt | 20 N·m | 15 lb ft
Seat Belt to Lower Center Pillar Bolt | 35 N·m | 26 lb ft
Seat Belt to Rear Seat Backrest Bolt | 40 N·m | 30 lb ft
Seat Belt to Upper Center Pillar Bolts | 35 N·m | 26 lb ft
Sunshade Bracket Bolts | 2.2 N·m | 19 lb in