For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Airbag Bolt - Side | 5 N·m | 44 lb in
Airbag Control Unit Nuts | 10 N·m | 89 lb in
Airbag Module Bolt | 5 N·m | 44 lb in
Airbag Sensor Bolt | 6 N·m | 53 lb in
Airbag Unit Bolt | 5 N·m | 44 lb in
Battery Bolt | 5 N·m | 44 lb in
Center Pillar Bolt - Upper and Lower | 2.5 N·m | 22 lb in
Front Seat Belt Bolt | 20 N·m | 15 lb ft
Front Seat Rear Bolts | 35 N·m | 26 lb ft
Height Adjuster Bolts | 35 N·m | 26 lb ft
Inner Panel Bolt | 2 N·m | 18 lb in
Instrument Panel Compartment Bolts | 4 N·m | 35 lb in
Instrument Panel Padding Bolts | 2.5 N·m | 22 lb in
Outer Panel Bolts | 2 N·m | 18 lb in
Rear Seat Backrest Front Bolts | 35 N·m | 25 lb ft
Rear Seat Backrest Rear Bolts | 35 N·m | 25 lb ft
Resonator Bolt | 2.5 N·m | 22 lb in
Roof Side Rail Modules Screws | 1.5 N·m | 13 lb in
Roof Side Rail Restraint Modules Screws | 1.5 N·m | 13 lb in
Seat Backrest Bolts - Front | 35 N·m | 26 lb ft
Seat Backrest Bolts - Rear | 25 N·m | 18 lb ft
Seat Belt Center Pillar Height Adjuster | 20 N·m | 15 lb ft
Seat Belt Reel Retractor Nut | 20 N·m | 15 lb ft
Seat Frame Bolts | 25 N·m | 18 lb ft
Side Airbag Sensor Bolts | 6 N·m | 53 lb in
Steering Wheel Coil Module Bolts | 15 N·m | 11 lb ft
Steering Wheel to Steering Column Bolt | 30 N·m | 22 lb ft
Turn Signal Switch Paneling Bolts | 15 N·m | 11 lb ft
Upper Paneling Bolts | 15 N·m | 11 lb ft