For 1990-2009 cars

# Information on Battery Label - Cold Cranking Amperage (CCA) Specification Required for Battery Testing

Subject: | Information on Battery Label -- Cold Cranking Amperage (CCA) Specification Required for Battery Testing

Models: | 2008 Saturn ASTRA

The purpose of this bulletin is to inform Saturn Retailers that the 300A (DIN) specification provided on the battery label relates to a European rating.

This value converts to 530 CCA under North American guidelines. Please use this information when performing a battery test.