SMU - Revised Engine Torque Specification Table. Saturn L Series 2001

For 1990-2009 cars

# SMU - Revised Engine Torque Specification Table

Subject: | Service Manual Update -- Revised Engine Torque Specification Table

Models: | 2000 and 2001 Saturn L-Series Vehicles

| with 3.0L V6 Engine (VIN R -- RPO L81)

Attention: | Technician

### Purpose

The purpose of this bulletin is to replace the torque table on page 34 of the 2000 Saturn L-Series Engine (L81) Service Manual and on page 36 of the 2001 Saturn L-Series Engine (L81) Service Manual with the table in this bulletin.

The eSI website will be updated immediately and future Service Stall SI CD releases will include this and other Service Manual updates.

APPLICATION | Nm | FT-LBS
--- | --- | ---
Camshaft Gear Bolt | 50+60°+15° | 37+60°+15°
Connecting Rod Bolt | 34+45°+15° | 26+45°+15°
Crankshaft Bearing Cap Bolts (Inner Bridge Bolts) | 60+15° | 44+15°
Crankshaft Drive Gear Bolt | 250+45°+15° | 184+45°+15°
Cylinder Head Bolt | 25+90°+90°+90°+15° | 18+90°+90°+90°+15°