For 1990-2009 cars

#### I/P Cluster Telltales and Indicators

(1) | Air Bag Readiness
(2) | Safety Belt Reminder
(3) | Low Fuel
(4) | MIL Service Engine Soon
(5) | Service Wrench
(6) | Washer Fluid Low
(7) | *Daytime Running Lamps (DRL)
(8) | *Left Turn Signal
(9) | *High Beam
(10) | *Right Turn Signal
(11) | Engine Oil Pressure
(12) | Antilock Brake System (ABS)
(13) | Charging System
(14) | Engine Coolant Temperature Warning
(15) | Reduced Power (V6 Only)
(16) | Low Traction
(17) | Brake System Warning
(18) | Change Oil Soon
(19) | Decklid/Liftgate Ajar
(20) | Shift Up, Manual Trans Only
(21) | Low Coolant Warning
(22) | Security

*Indicator uses replaceable bulb.

The daytime running lamps (DRL) indicator, high beam indicator and turn signal indicators all use replaceable bulbs, blue base. All other telltales utilize LEDs which are not replaceable. Additionally, the instrument cluster contains six replaceable bulbs, blue base, for illumination and one replaceable bulb, white base, for odometer backlighting.

#### Replacement Bulbs

(1) | Instrument Cluster Illumination (6 Bulbs)
(2) | Turn Signal Indicators
(3) | Daytime Running Lamps (DRL) Indicator
(4) | Odometer Backlighting
(5) | High Beam Indicator