For 1990-2009 cars

### What to Use

When you need windshield or rear window (wagon models) washer fluid be sure to read the instructions before use. If you will be operating your vehicle in an area where the temperature may fall below freezing, use a fluid that has sufficient protection against freezing.

### Adding Windshield Washer Fluid

Open the cap with the washer fluid symbol printed on it and add washer fluid until the tank is full.

Notice:

• | When using concentrated washer fluid, follow the manufacturer's instructions for adding water.

• | Do not mix water with ready-to-use washer fluid. Water can cause the solution to freeze and damage your washer fluid tank and other parts of the washer system. Also, water does not clean as well as washer fluid.

• | Fill the washer fluid tank only three-quarters full when it is very cold. This allows for fluid expansion if freezing occurs, which could damage the tank if it is completely full.

• | Do not use engine coolant (antifreeze) in your windshield washer. It can damage the vehicle's windshield washer system and paint.