For 1990-2009 cars

Torque Specification Description | Specification
--- | ---
Metric | English
B-Pillar Molding Fastener | 10 N·m | 89 lb in
Child Restraint Bracket Bolt | 20 N·m | 15 lb ft
Console Screws | 1.2 N·m | 11 lb in
Front Seat Anchoring Bolts | 20 N·m | 15 lb in
Height Adjuster Fasteners | 35 N·m | 26 lb ft
Inflator Fasteners | 5 N·m | 18 lb ft
Passenger Inflator Module (Air Bag) Bolts | 10 N·m | 89 lb ft
Rear Retractor-to-Vehicle Bolt | 35 N·m | 26 lb ft
Rear Shoulder Belt-to-C-Pillar Bolt | 35 N·m | 26 lb ft
Rear Shoulder Belt-to-Floor Bolt | 35 N·m | 26 lb ft
Retractor Fastener | 35 N·m | 26 lb ft
Sensing Diagnostic Module Nuts | 10 N·m | 89 lb in
SIS Fasteners | 10 N·m | 89 lb in
Safety Belt Guide Fasteners | 1.5 N·m | 13 lb in
Seat Belt Buckle-to-Seat Frame Fasteners | 35 N·m | 26 lb ft
Seat Center Seat Belt Bolts | 35 N·m | 26 lb ft
Shoulder Belt-to-Height Adjuster Bolt | 29 N·m | 21 lb ft
Shoulder Belt-to-Seat Track Fastener | 20 N·m | 15 lb ft
Steering Column Cover Fasteners | 4 N·m | 35 lb in
Steering Wheel Nut | 10 N·m | 30 lb in