For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) trim panel. Refer to Instrument Panel Center Trim Panel Replacement .
2. Release the tabs and push on the switch from the back side of the panel.
3. Remove the switch (1).

### Installation Procedure

1. Install the switch (1) into the opening.
2. Press on the switch (1) assembly until fully seated.
3. Install the I/P trim panel. Refer to Instrument Panel Center Trim Panel Replacement .