For 1990-2009 cars

Torque Spec Description | Specification
--- | ---
Metric | English
Assist Handle Bracket-to-Roof Rail Bolts | 16 N·m | 12 lb ft
B-Pillar Fastener | 10 N·m | 89 lb in
B-Pillar Molding Fastener | 10 N·m | 89 lb in
Child Restraint Bracket Bolt | 20 N·m | 15 lb ft
Console Screws | 1.2 N·m | 11 lb in
Curtain Inflator Retaining Bolt (10 mm Hex Head) | 10 N·m | 89 lb in
Curtain Inflator Retaining Nut (10 mm Hex Head) | 10 N·m | 89 lb in
Curtain Inflator Retaining Screw (7 mm Hex Head) | 2.5 N·m | 22 lb in
Front Seat Anchoring Bolts | 20 N·m | 15 lb ft
Height Adjuster Fasteners | 35 N·m | 26 lb ft
Inflator Fasteners | 5 N·m | 18 lb in
Knee Bolster Bolts | 2.3 N·m | 20 lb in
Latch Bracket Attaching Bolts | 25 N·m | 18 lb ft
Passenger Inflator Module (Air Bag) Bolts | 10 N·m | 89 lb in
Rear Retractor-to-Vehicle Bolt | 35 N·m | 26 lb ft
Rear Seat Belt Shoulder Belt-to-C-Pillar | 35 N·m | 26 lb ft
Rear Seat Center Belt Buckle Fastener | 35 N·m | 26 lb ft
Rear Seat Shoulder Belt Retractor | 35 N·m | 26 lb ft
Rear Shoulder Belt-to-C-Pillar | 35 N·m | 26 lb ft
Rear Shoulder Belt-to-C-Pillar Bolt | 35 N·m | 26 lb ft
Rear Shoulder Belt-to-Floor Bolt | 35 N·m | 26 lb ft
Retractor Fastener | 35 N·m | 26 lb ft
SDM Nuts | 10 N·m | 89 lb in
SIS Fasteners | 10 N·m | 89 lb in
Safety Belt Guide Fasteners | 1.5 N·m | 13 lb in
Seat Belt Buckle-to-Seat Frame Fasteners | 35 N·m | 26 lb ft
Seat Center Seat Belt Bolts | 35 N·m | 26 lb ft
Shoulder Belt-to-Height Adjuster Bolt | 29 N·m | 21 lb ft
Shoulder Belt-to-Seat Track Fastener | 20 N·m | 15 lb ft
Steering Column Cover Fasterns | 4 N·m | 35 lb in
Steering Wheel Nut | 40 N·m | 30 lb ft