For 1990-2009 cars

The following table lists the parameters displayed by the Scan tool. The parameters are displayed by ABS/TCS data, switch inputs, exterior lamps, interior lamps, door locks, wiper/washer and security data groups.

#### ABS/TCS Data Scan Tool Data List

Scan Tool Parameter | Units Displayed
--- | ---
Battery 1 | Volts
Traction Active | Yes/No
Traction Control Status | On/Off
ABS Fault | Yes/No
Traction LED Command | On/Off
Traction LED Feedback | High/Low
Park Brake Switch | On/Off
Fuel Gauge Position | %
Coolant Gauge Position | %
Displayed Odometer | km/miles

#### Switch Inputs Scan Tool Data List

Scan Tool Paramter | Units Displayed
--- | ---
Battery 1 | Volts
Driver Door Switch | High/Low
Pass. Door Switches | High/Low
Key In Ignition | Yes/No
Decklid Ajar Switch | High/Low
Oil Life Reset Switch | High/Low
Park Brake Switch | On/Off
Low Coolant | Yes/No
Low Brake Fluid | Yes/No
A/C Request (RPO C60) | Yes/No
High Beam Input = Off (2002) | Yes/No
High Beam Input = DRL (2002) | Yes/No
High Beam Input = High (2002) | Yes/No
Low Beam Input = Off (2003) | Yes/No
Low Beam Input = DRL (2003) | Yes/No
Low Beam Input = High (2003) | Yes/No
Low Beam Switch | On/Off
Parklamp Switch | On/Off
Lock Switch | On/Off
Unlock Switch | On/Off
Front Wiper Switch | On/Off
Rear Wiper Switch | On/Off
Rear Defog Switch (RPO C60) | On/Off
Rear Defog Relay Cmd. | On/Off
Rear Defog Relay Fdbk. | High/Low
Shifter Unlock Cmd. | On/Off
Shifter Unlock Fdbk. | High/Low

#### Exterior Lamps Scan Tool Data List

Scan Tool Parameter | Units Displayed
--- | ---
Battery 1 | Volts
High Beam Input = Off (2002) | Yes/No
High Beam Input = DRL (2002) | Yes/No
High Beam Input = High (2002) | Yes/No
Low Beam Input = Off (2003) | Yes/No
Low Beam Input = DRL (2003) | Yes/No
Low Beam Input = High (2003) | Yes/No
Low Beam Switch | On/Off
Parklamp Switch | On/Off
DRL Relay Command | On/Off
DRL Relay Feedback | High/Low
ALC Light Sensor | Volts
Parklamp Input | Volts
Parklamp Cmd. | On/Off
Parklamp Fdbk. | High/Low
Headlamp Cmd. | On/Off
Headlamp Fdbk. | High/Low

#### Interior Lamps Scan Tool Data List

Scan Tool Parameter | Units Displayed
--- | ---
Battery 1 | Volts
Inadvertent Power Cmd. | On/Off
Inadvertent Power Fdbk. | High/Low
Dome Lamp Command | On/Off
Dome Lamp Feedback | High/Low
Driver Door Switch | High/Low
Pass. Door Switches | High/Low
Key In Ignition | Yes/No
I/P Dimmer Input | Volts
I/P Dimmer Output | % Duty Cycle

#### Door Locks Scan Tool Data List

Scan Tool Parameter | Units Displayed
--- | ---
Battery 1 | Volts
Driver Unlock Relay Cmd. | On/Off
Driver Unlock Relay Fdbk. | High/Low
Pass. Unlock Relay Cmd. | On/Off
Pass. Unlock Relay Fdbk. | High/Low
Lock All Relay Cmd. | On/Off
Lock All Relay Fdbk. | High/Low
Remote Lock Command | Yes/No
Remote Unlock Command | Yes/No
Remote Panic Command | Yes/No
Remote Trunk Command | Yes/No
Lock Switch | On/Off
Unlock Switch | On/Off
Trunk Release Switch | On/Off
Trunk Release Sol. Cmd. | On/Off
Trunk Release Sol. Fdbk. | High/Low

#### Wiper/Washer Scan Tool Data List

Scan Tool Parameter | Units Displayed
--- | ---
Battery 1 | Volts
Wiper Delay Input | Volts
Wiper Delay 1 | Yes/No
Wiper Delay 2 | Yes/No
Wiper Delay 3 | Yes/No
Front Wiper Switch | On/Off
Front Wiper Relay Cmd. | On/Off
Front Wiper Relay Fdbk. | High/Low
Rear Wiper Switch | On/Off
Rear Wiper Relay Cmd. | On/Off
Rear Wiper Relay Fdbk. | High/Low
Front Washer Motor Input | On/Off
Rear Washer Motor Input | On/Off
Washer Fluid Level | Low/OK

#### Security Data Scan Tool Data List

Scan Tool Parameter | Units Displayed
--- | ---
Battery 1 | Volts
Ignition 1 Input | High/Low
Accessory | High/Low
Passlock Input | Volts
Passlock Power Fdbk. | High/Low
Key Learn Enabled | Yes/No
Security LED | On/Off/Flash
Horn Relay Command | On/Off
Horn Relay Feedback | High/Low
Passlock Timer | Seconds
Auto-Learn Timer | Seconds
Decklid Ajar Switch | High/Low
Trunk Release Switch | On/Off