For 1990-2009 cars

### Removal Procedure

Important: The AM/FM stereo with cassette and in-dash CD player shown, knobs for AM/FM stereo with cassette player/6-disc in-dash CD player and AM/FM stereo with in-dash CD player, are similar.

Remove the desired knob, VOL (1) or BASS/TREB/FADE/BAL (2), from the radio by pulling straight out on the knob.

### Installation Procedure

Install the desired knob to the radio by placing the knob over its post and pushing the knob onto the radio.