For 1990-2009 cars

#### Direct Clutch Plate Selection Specifications

Broadcast Codes | Quantity
--- | ---
Steel | Fiber
WXJ | 6 | 6
WCR | 6 | 6
MXJ | 6 | 6
FDJ | 6 | 6
PCR | 7 | 5

#### Reverse Clutch Backing Plate Specifications

Recorded Measurement | Backing Plate Identification
--- | ---
8.970-9.433 mm (0.353-0.371 in) | A

#### Direct Clutch Plate Selection Specifications

Broadcast Codes | Quantity
--- | ---
Steel | Fiber
WXJ | 6 | 6
ERJ | 6 | 6
ESJ | 6 | 6
ETJ | 6 | 6
EVJ | 6 | 6
EBJ | 7 | 5
MXJ | 6 | 6
PCR | 7 | 5
EHJ | 7 | 5
FWJ | 7 | 6