For 1990-2009 cars

Your vehicle is equipped with a split folding rear seat. A split folding rear seat enables you to carry long cargo by folding down part or all of the rear seat.

### Sedan

On sedans, you can fold either the driver's or passenger's right side of the seatback separately or both sides together. Lift the lever on the corner of the seatback.

When you fold the seatback up, be sure the latches engage by pushing rearward with your hand over the latch locations. Then push and pull at the top of the seatback to ensure that all latches are secure.

### Wagon

On wagons, you can fold either the passenger's side of the seatback or the entire seatback.

To fold down the passenger's side of the seatback, pull the lever on the corner of the passenger's side seatback. To lower the entire rear seatback, pull the lever on the corner of the driver's side seatback.

Caution: If either seatback is not locked, it could move forward in a sudden stop or crash. That could cause injury to the person sitting there. Always push and pull on the seatbacks to be sure they are locked.

When the seatback is put in an upright position, be sure the latches engage by pushing rearward with your hand over the latch locations. Then push and pull at the top of the seatback to ensure that all latches are secure.