For 1990-2009 cars

# Service Information to Provide New Procedure, Labor Operation Code, and Parts Information for Drivers Side Floor Mat Retainer

Subject: | Service Information to Provide New Procedure, Labor Operation Code, and Parts Information for "Driver's Side Floor Mat Retainer"

Models: | 2000 - 2001 Saturn L-Series Vehicles

### PURPOSE

The purpose of this bulletin is to:

Provide a new "Driver's Side Floor Mat Retainer " procedure and to update all 2000 and 2001 L-Series Body/Electrical Volume II Service Manuals and update as detailed:

• | In the 2000 -- L-Series Body/Electrical Volume II Service Manual, insert a copy of page 2 of this bulletin between service manual pages 1012 and 1013.

• | In the 2001 L-Series Body/Electrical Volume II Service Manual, insert a copy of page 2 of this bulletin between service manual pages 1034 and 1035.

Provide new labor code C4219 in order to receive credit for this repair during the warranty period.

Service Manual update page to be inserted in the 2000 and 2001 L-Series Body/Electrical Volume II Service Manuals. Refer to Technical Information Bulletin 00-T-69. December 2000

### DRIVER'S SIDE FLOOR MAT RETAINER

1. Remove the driver's side floor mat.
2. Remove floor mat retainer using screwdriver inserted into top slot retainer.
3. Screw in new retainer and snap floor mat into place.

#### Parts Requirement:

Parts Number | Color | Description
--- | --- | ---
222676899 | Ebony | Retainer-FLR MAT
22676901 | MD DK OAK | Retainer-FLR MAT
22676902 | MD PTR II | Retainer-FLR MAT

### CLAIM INFORMATION

To receive credit for this repair during the warranty coverage period, submit a claim through the Saturn Dealer System C4219, (Retainer, Floor Mat, Left - Replace.