For 1990-2009 cars

## Cargo Lamp Replacement Wagon

### Removal Procedure

1. Using a small flat blade screwdriver, carefully remove rear cargo lamp assembly.
2. Using a towel to hold bulb, gently pull on bulb to remove cargo lamp bulb from cargo lamp.

### Installation Procedure

1. Using a towel to hold bulb, install cargo lamp bulb into cargo lamp assembly.
2. Snap cargo lamp assembly into headliner assembly.