For 1990-2009 cars

# Service Information Regarding Engine Support During Removal of Right Front Engine Mount Assembly

Subject: | Service Information Regarding Engine Support During Removal of Right Front Engine Mount Assembly

Models: | 2000-2005 Saturn L-Series

| 2002-2003 Saturn VUE

| with 3.0L V6 Engine (VINs R, B -- RPO L81)

Attention: | Technician

This bulletin is being updated to include the 2005 model year. Please discard Corporate Bulletin Number 04-06-01-004 (Section 06 -- Engine/Propulsion System).

### Purpose

The purpose of this bulletin is to provide updated information regarding engine support when removing the right front engine mount.

### Procedure

Notice: Use the listed tools, or equivalent, to properly support the engine assembly during the "Right Front Engine Mount Assembly" removal and installation procedures. Do NOT use a floor jack and block of wood to support the engine assembly. The engine oil pan is not designed to support engine weight and may cause oil pan damage.

1. Engine Support Adapter - J45122
2. Engine Support Fixture Legs - SA9105E
3. Engine Support Fixture Long Bar - SA9105E
4. Engine Support Cross Bar - SA9105E
5. Engine Support Fixture Hook (Front Only) - J43405 (J28467-A)
6. Engine Support Fixture Hook (Rear Only) - J44804
7. Engine Off-Set Bracket - J43405 (J28467-27A)
8. Engine Support Fixture Handle - J43405

1. Engine Support Fixture Legs - J43405 (J43405-1)
2. Engine Support Fixture Long Bar - SA9105E
3. Engine Off-Set Bracket - J43405 (J28467-27A)
4. Engine Support Fixture Handle - J43405
5. Engine Support Hook - J43405 (J28467-A)

1. Engine Support Fixture Adapter - J43405
2. Engine Support Fixture (3 Bar) - SA9105E