For 1990-2009 cars

### Power Driver Seat Control Switch

The power seat switch contains 3 switches to adjust the recliner, the head rest, and the bottom cushion height. The power seat adjuster switch is a 2-way (forward/backward) adjustment switch.

The power driver seat control switch is located on the left side of the seat cushion. With this control, the driver seat cushion can be moved up, down, forward, and rearward. The seat back portion of the seat can also be reclined or straight up. When a side of the up/down switch is pressed, the entire seat is accordingly raised or lowered. When the switch is moved forward or rearward, the seat is accordingly moved forward or rearward. When a side of the recline switch is pressed, the rear portion of the seat cushion is accordingly raised or reclined.