For 1990-2009 cars

### Removal Procedure

1. Remove the rear wiper arm finish cap.
2. Remove the wiper arm nut and washer.
3. Remove the rear wiper arm.

### Installation Procedure

1. Install the rear wiper arm.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the wiper arm washer and nut.

Tighten
Tighten the nut to 9 N·m (80 lb in).

3. Install the rear wiper arm finish cap.