For 1990-2009 cars

## Electrical Center Identification Views L61

Table 1: | Maxifuse/Minifuse Feeds
Table 2: | Relay Circuit Feeds
Table 3: | Misc Devices
Table 4: | Minifuse Circuit Feeds

### Underhood Fuse Block Diagram

### Underhood Fuse Block Charts

This chart lists the maxifuses and minifuses they control.

#### Maxifuse/Minifuse Feeds

NO. | FUSE (CB) | COLOR (AMP) | SYSTEM
--- | --- | --- | ---
1 | COOL FAN 1 | Green (30) | Cooling Fan Control Module
2 | COOL FAN 2 | Green (30) | Cooling Fan Control Module
3 | IGN 1/2 | Green (30) | Ignition Switch
4 | IGN 0/3/CR | Green (30) | Ignition Switch
5 | ABS I | Green (30) | Electronic Brake/Traction Control Module
6 | ABS II | Green (30) | Electronic Brake/Traction Control Module
7 | HVAC BLOWER AMBER | Green (30) | HVAC Blower Relay
8 | WDO/SUNROOF/AIR | Circuit Breaker (30) | Window Relay/Sunroof Assembly/Secondary Air

The following chart lists the relays located in the underhood fuse block, and the systems they control.

#### Relay Circuit Feeds

RELAY | MAXIMUM LOAD | SYSTEM
--- | --- | ---
DRL | 20 Amp | Daytime Running Lamps
HORN | 20 Amp | Horn
A/C | 20 Amp | A/C Compressor

The following chart lists the devices located in the underhood fuse block, and the systems they control.

#### Misc Devices

DEVICE | SYSTEM
--- | ---
Oil Life Reset | Body Control Module
A/C Diode | A/C Compressor
Fuse Puller | None

The following chart lists the minifuses located in the underhood fuse block, and the circuits they feed.

#### Minifuse Circuit Feeds

FUSE | COLOR (AMP) | SYSTEM
--- | --- | ---
LIGHTER | Yellow (20) | Cigar Lighter
LHDLP | Blue (15) | Left Headlamp - High and Low Beam
RHDLP | Blue (15) | Right Headlamp - High and Low Beam
BCM 2 | Red (10) | Body Control Module
IGN 3 | Red (10) | Evaporative Emission Canister Purge Solenoid/Cruise Clutch Switch/EVAP Vent Solenoid/Heat Oxygen Sensor 2
AUX | Yellow (20) | Auxiliary Power Outlet
RT IP BATT | Green (30) | Door Locks/Heat Mirror Relay/Power Seat/Premium Sound Amplifier/Fog Lamp Relay
CONTROL B+ | Red (10) | Powertrain Control Module
HORN | Red (10) | Horn Relay
FUEL PUMP | Blue (15) | Fuel Pump Relay
A/C | Red (10) | A/C Relay
IGN 0 | Red (10) | Powertrain Control Module
RR DEFOG | Natural (25) | Rear Defog Relay
BCM/ECM/CRUISE/ABS | Red (10) | Electronic Brake/Traction Control Module/Cruise Control Module/Body Control Module/Cruise Brake Switch/Cruise Switch Fuse
CRUISE SW | Grey (2) | Horn/Cruise Switch
INJ | Red (10) | Fuel Injectors
CONTROLS IGN 1 | Red (10) | Powertrain Control Module/Cooling Fan Control Module/Automatic Transaxle
HAZARD | Blue (15) | Hazard Switch
IGN 1 | Red (10) | I/P Cluster/Coolant Level Switch/Electronic PRNDL Module/Sensing and Diagnostic Module
BRAKE | Blue (15) | Stop Lamp Switch
PARK LP | Red (10) | Headlamp/Turn Signal Switch
EIS | Red (10) | Electronic Ignition Module
BU/TURN | Red (10) | Park/Neutral Position Switch/Back-Up Switch/Hazard Switch
BCM/CLUSTER | Blue (15) | Body Control Module/I/P Cluster/Decklid Release/Dimmer Switch
RADIO | Red (10) | Radio
CD/DLC | Blue (15) | Data Link Connector/Radio

## Electrical Center Identification Views L81

Table 1: | Maxifuse/Minifuse Feeds
Table 2: | Relay Circuit Feeds
Table 3: | Misc Devices
Table 4: | Minifuse Circuit Feeds

### Underhood Fuse Block Diagram

### Underhood Fuse Block Charts

This chart lists the maxifuses and minifuses they control.

#### Maxifuse/Minifuse Feeds

NO. | FUSE (CB) | COLOR (AMP) | SYSTEM
--- | --- | --- | ---
1 | COOL FAN 1 | Green (30) | Cooling Fan Control Module
2 | COOL FAN 2 | Green (30) | Cooling Fan Control Module
3 | IGN 1/2 | Green (30) | Ignition Switch
4 | IGN 0/3/CR | Green (30) | Ignition Switch
5 | ABS I | Green (30) | Electronic Brake/Traction Control Module
6 | ABS II | Green (30) | Electronic Brake/Traction Control Module
7 | HVAC BLOWER | Green (30) | HVAC Blower Relay
8 | WDO/SUNROOF/AIR | Circuit Breaker (30) | Window Relay/Sunroof Assembly

The following chart lists the relays located in the underhood fuse block, and the systems they control.

#### Relay Circuit Feeds

RELAY | MAXIMUM LOAD | SYSTEM
--- | --- | ---
DRL | 20 Amp | Daytime Running Lamps
MAIN | 20 Amp | Engine Control 1/2/3 Fuses
HORN | 20 Amp | Horn
A/C | 20 Amp | A/C Compressor

The following chart lists the devices located in the underhood fuse block, and the systems they control.

#### Misc Devices

DEVICE | SYSTEM
--- | ---
Oil Life Reset | Body Control Module
A/C Diode | A/C Compressor
Fuse Puller | None

The following chart lists the minifuses located in the underhood fuse block, and the circuits they feed.

#### Minifuse Circuit Feeds

FUSE | COLOR (AMP) | SYSTEM
--- | --- | ---
LIGHTER | Yellow (20) | Cigar Lighter
LHDLP | Blue (15) | Left Headlamp - High and Low Beam
RHDLP | Blue (15) | Right Headlamp - High and Low Beam
BCM2 | Red (10) | Body Control Module
ENG CNTL 1 | Red (10) | A/C Relay, Mass Airflow Sensor, Evaporative Emission Canister Purge Solenoid, Heated Oxygen Sensor Bank 2, Sensors 1 and 2 Linear Exhaust Gas Recirculation Valve
ENG CNTL 2 | Red (10) | Fuel Injectors, Variable Intake Manifold Solenoid
AUX | Yellow (20) | Auxiliary Power Outlet
RT IP BATT | Green (30) | Door Locks/Heat Mirror Relay/Power Seat/Premium Sound Amplifier/Fog Lamp Relay
ENG CNTL 3 | Green (30) | Heated Oxygen Sensor Bank 1 Sensors 1 and 2, Engine Control Module Fuel Pump Relay, EVAP Vent Solenoid
CONTROLS B+ | Red (10) | Engine Control Module/Transmission Control Module
HORN | Red (10) | Horn Relay
FUEL PUMP | Blue (15) | Fuel Pump Relay
A/C | Red (10) | A/C Relay
IGN 0 | Red (10) | Park/Neutral Position Switch/Park Lock/PRNDL/PCM
RR DEFOG | Natural (25) | Rear Defog Relay
BCM/ECM/CRUISE/ABS | Red (10) | Electronic Brake/Traction Control Module/Engine Control Module/Body Control Module/Cruise Brake Switch/Cruise Switch Fuse
CRUISE SW | Grey (2) | Horn/Cruise Switch
CONTROLS IGN 1 | Red (10) | Transaxle Control Module/Cooling Fan Control Module
HAZARD | Red (10) | Hazard Switch
IGN 1 | Red (10) | I/P Cluster/Coolant Level Switch/Electronic PRNDL Module/Sensing and Diagnostic Module
BRAKE | Blue (15) | Stop Lamp Switch
PARK LP | Red (10) | Headlamp/Turn Signal Switch
IGN | Blue (15) | Ignition Coils
BU/TURN | Red (10) | Park/Neutral Position Switch/Coolant Flow Pump/Hazard Switch
BCM/CLUSTER | Blue (15) | Body Control Module/I/P Cluster/Decklid Release/Dimmer Switch
Radio | Red (10) | Radio
CD/DLC | Blue (15) | Data Link Connector/Radio

## Electrical Center Identification Views Left

Table 1: | Minifuse Circuit Feeds
Table 2: | Relay/Module Circuit Feeds
Table 3: | Misc Devices

### Instrument Panel Fuse Block Diagram

### Instrument Panel Fuse Block Charts

The following chart lists the minifuses located in the left instrument panel fuse block, and the systems they control.

#### Minifuse Circuit Feeds

FUSE | COLOR (AMP) | SYSTEM
--- | --- | ---
RADIO | Red (10) | Radio
BTSI/BCM/MIRROR | Red (10) | BTSI Solenoid/Parklock Switch/Body Control Moudle/Power Mirror Switch
WIPER | Natural (25) | Wiper Relay/Wiper Switch/Front Wiper Motor
DEFOG LED | Red (10) | Rear Defog Switch
IGN 3 | Red (10) | Rear Defog Relay/HVAC Control Head/Vehicle Speed Signal Conditioner Module/Traction Control/Passenger Heated Seat Switch/Fog Lamp/Driver Heated Seat Switch
HVAC SW | Yellow (20) | HVAC Control Head
DIMMER | Red (10) | Dimmer

The following chart lists the devices located in the left fuse block, and the systems they control.

#### Relay/Module Circuit Feeds

RELAY | MAXIMUM LOAD | SYSTEM
--- | --- | ---
WIPER | 20 Amp | Wiper Switch/Wiper Motor
RR DEFOGGER | 20 Amp | Rear Defog Switch/Rear Defog Grid
FUEL PUMP | 20 Amp | Fuel Pump
HVAC BLOWER | 35 Amp | HVAC Control Head/Blower Motor

The following chart lists the devices located in the left instrument panel fuse block and the systems they control.

#### Misc Devices

DEVICE | SYSTEM
--- | ---
RR Comp Diode | Liftgate/Decklid Ajar Switch
Fuse Puller | None

## Electrical Center Identification Views Right

Table 1: | Minifuse Circuit Feeds
Table 2: | Relay/Module Circuit Feeds
Table 3: | Misc Devices

### Instrument Panel Fuse Block Diagram

### Instrument Panel Fuse Block Charts

The following chart lists the minifuses located in the left instrument panel fuse block, and the systems they control.

#### Minifuse Circuit Feeds

FUSE | COLOR (AMP) | SYSTEM
--- | --- | ---
LOCKS | Blue (15) | Door Lock/Unlock Relays
PWR SEAT | Yellow (20) | Drivers Power Seat Switch
BODY | Red (10) | Heated Mirror Relay/Liftgate Key Cylinder Switch/Door Lock Switch
FOG LP | Red (10) | Fog Lamp Relay
PREM AMP | Blue (15) | Amplifier
HEATED SEATS | Yellow (20) | Heated Seat
WIPER/SUNROOF | Yellow (20) | Rear Wiper Relay/Rear Wiper Motor/Sunroof Assembly

The following chart lists the devices located in the left fuse block, and the systems they control.

#### Relay/Module Circuit Feeds

RELAY | MAXIMUM LOAD | SYSTEM
--- | --- | ---
DR UNLOCK | 20 Amp | Door Lock Motor
UNLOCK | 20 Amp | Door Lock Motor
LOCK | 20 Amp | Door Lock Motor
MIRROR | 20 Amp | Mirror Switch/Mirror
FOG LAMP | 20 Amp | Fog Lamp Switch/Fog Lamps
RR WIPER | 20 Amp | Rear Wiper Switch/Rear Wiper Motor
WINDOWS | 35 Amp | Window Switch/Sunroof Assembly

The following chart lists the devices located in the left instrument panel fuse block and the systems they control.

#### Misc Devices

DEVICE | SYSTEM
--- | ---
Fuse Puller | None