For 1990-2009 cars

You can tow your Saturn behind another vehicle for use at your destination. Be sure to use the proper towing equipment designed for recreational vehicle towing. Follow the instructions for the equipment.

### Towing Your Vehicle from the front

There are two ways to tow your vehicle from the front.

To tow your vehicle with a dolly, do follow these steps:

1. Put the front wheels on a dolly.
2. Move the shift to "P" (Park).
3. Set the parking brake and then remove the key.
4. Clamp the steering wheel in a straight-ahead position with a clamping device designed for towing.
5. Release the parking brake.

### Towing your Vehicle with All Four Wheels on the Ground

To tow your vehicle will all four wheels on the ground, follow these steps:

1. Position and attach vehicle to tow it behind the recreational vehicle.
2. Turn the ignition key to "OFF" position.
3. Secure the vehicle.
4. Turn the ignition key to "ACC" position.
5. Turn the fog lamps and all accessories off.
6. Shift the transaxle to "N" (Neutral).
7. Release the parking brake.

### Towing Your Vehicle from the Rear