For 1990-2009 cars

## Diagnostic System Check - Lighting Systems without Fog Lamps

Action | Normal Results
--- | ---

• | Start engine and allow to idle in PARK.

| Start engine and allow to idle in NEUTRAL (w/manual transaxle).

• | Apply park brake.

High beam and Low beam headlamps are OFF. Daytime running lamps indicator is OFF.

• | Release park brake.

• | Move transaxle out of PARK (Automatic).

Headlamps are ON at reduced brilliance (DRL Mode). Daytime running lamps indicator is ON.

• | Move headlamp dimmer switch to LOW.

• | Turn headlamp switch to HEAD.

High beam headlamps are OFF. Low beam headlamps are ON. Daytime running lamps indicator is OFF.

Move headlamp dimmer switch to HIGH. | High beam headlamps and high beam indicator are ON. Low beam headlamps are OFF. Daytime running lamps indicator is OFF.
Turn headlamp switch to OFF. | Headlamps are ON at reduced brilliance. Daytime running lamps indicator is ON during the day with the A/C OFF.
Turn ignition switch to OFF. | Headlamps are OFF.
Move headlamp switch to PARK. | Park lamps are ON. Headlamps are ON at reduced brilliance (DRL mode).
The daytime running will operate normally during the day.

## Diagnostic System Check - Lighting Systems with Fog Lamps

Action | Normal Results
--- | ---

• | Start engine and allow to idle.

• | Move gear selector to any position except PARK.

• | Fog lamp switch is OFF.

• | Apply park brake.

Fog lamps, high beam headlamps and low beam headlamps are OFF. Daytime running lamps indicator is OFF.

Release park brake. | Headlamps and fog lamps are OFF. Headlamps are ON at reduced brilliance (DRL mode). Daytime running lamps indicator is ON.

• | Move headlamp switch to HEAD.

• | Move fog lamp switch ON.

• | Headlamp dimmer switch in HIGH.

High beam headlamps and high beam indicator are ON. Low beam headlamps and fog lamps are OFF.

• | Move headlamp dimmer switch to LOW.

• | Move fog lamp switch ON.

Low beam headlamps and fog lamps are ON. High beam headlamps and high beam indicator are OFF.

• | Move headlamp switch to PARK.

• | Fog lamp switch still ON.

Headlamps are OFF. Fog lamps are ON.

Turn ignition switch OFF. | Headlamps and fog lamps are OFF.