For 1990-2009 cars

#### Auxiliary Power Outlet -- Rear Console

Connector Part Information |

• | 12176446

• | Black

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | ORN | 1740 | Auxiliary Fuse
B | -- | -- | Not Used
C | BLK | 550 | Center Console Ground

#### I/P Fuse Block - Left - Body -- Left Kick Panel

Insert Graphic SMELC80249AB2
Connector Part Information |

• | 15326717

• | Gray

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1 | BLK | 550 | Ground
A2 | BRN | 9 | Park Lamp
A3 | BLK/WHT | 56 | Valet Switch (Sedan)
BLK | 305 | Liftgate (Wagon)
A4 | YEL | 743 | Power Mirror
A5 | -- | -- | Not Used
A8 | PPL | 30 | Fuel Tank Inline
A9 | LT BLU | 14 | Left Rear Turn Lamp
A10 | LT BLU | 20 | Rear Lamps
A11 | -- | -- | Not Used
A12 | PPL | 293 | Rear Defog
B1 | BLK | 550 | Mirror Switch - Mirror Motor
B2 | BRN | 9 | License Lamp
B3 | -- | -- | Not Used
B4 | LT GRN | 24 | Back-Up Lamp
B5 | ORN | 1732 | Cargo Lamp (Sedan) Headliner (Wagon)
B8 | WHT | 1310 | Vent Solenoid
B9 | DK BLU | 15 | Right Rear Turn Lamp
B10 | LT BLU | 20 | Headliner - CHMSL
B11 | ORN | 393 | Rear Wiper (Wagon)
B12 | LT BLU | 82 | Mirrors
C1 | ORN | 2740 | Vent Solenoid
C2 | GRY/BLK | 745 | Left Front Door Jamb
C3 | -- | -- | Not Used
C4 | TAN | 638 | RIPFB
C5 | ORN | 1732 | Left Front Door Left Rear Door
C8 | BLK | 1576 | Valet Switch
C9 | WHT | 1310 | Fuel Tank Inline
C10 | -- | -- | Not Used
C11 | BLK | 2759 | Fuel Tank Inline
C12 | LT BLU | 82 | Mirror Switch

#### I/P Fuse Block - Left - I/P -- Left Kick Panel

Insert Graphic SMELC80214AB1
Connector Part Information |

• | 15303512

• | Gray

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1 | BLK | 550 | Horn/Key Chime
A2 | -- | -- | Not Used
A3 | BLK/WHT | 56 | BCM
A4 | GRY | 8 | HVAC - Hazard Switch
A5 | GRY | 8 | Decklid Release - Dimmer
A6 | GRY | 8 | Cigar Lighter - PRNDL
A7 | PPL | 1319 | Engine to I/P Inline (L81)
A8 | -- | -- | Not Used
A9 | LT BLU | 14 | Hazard Switch - Left Turn Telltale
A10 | BLK | 2754 | Engine to I/P Inline
A11 | RED | 502 | Ignition 3 Relay
A12 | ORN | 300 | Ignition Switch - RIPFB
B1 | BLK | 550 | Glove Box Lamp - Hazard Switch
B2 | -- | -- | Not Used
B3 | YEL | 343 | UHFB
B4 | ORN | 1732 | BCM - Glove Box
B5 | GRY | 8 | Cluster - Radio
B6 | GRY | 8 | Traction Switch - Heated Seat Switch - Fog Lamp Switch
B7 | PPL | 1319 | DLC (L81)
B8 | -- | -- | Not Used
B9 | LT BLU | 4 | UHFB - Left Turn Switch
B10 | DK BLU | 15 | Right Turn Switch - Right Hazard Switch
B11 | BLK | 550 | PRNDL - Vehicle Speed Signal Modifier (L81)
B12 | ORN | 300 | UHFB (L61)
C1-C2 | -- | -- | Not Used
C3 | YEL | 343 | Wiper Switch
C4 | BRN | 9 | UHFB
C5 | ORN | 1732 | Body to I/P Inline - Right
C6-C7 | -- | -- | Not Used
C8 | GRN | 120 | UHFB
C9 | -- | -- | Not Used
C10 | DK BLU | 15 | Park Lock - BTSI - PRNDL
C11 | BLK | 550 | HVAC - Brake Fluid
C12 | YEL | 268 | HVAC Module
D1 | BLK | 550 | Wiper Switch
D2 | BRN | 1341 | UHFB
ORN | 2740 | UHFB
D3 | YEL | 343 | Engine to I/P Inline
D4 | BRN | 9 | PRNDL - RIPFB
D5-D8 | -- | -- | Not Used
D9 | BLK | 550 | Park Lock - BTSI - PRNDL
D10 | BLK | 2759 | Engine to I/P Inline (L81) Pedal Position Switch (L81)
D11 | BLK | 550 | Traction Heated Seat switch Fog Lamp Switch
D12 | PNK | 393 | UHFB
E1 | BLK | 550 | Decklid Release/Dimmer/Headlamp Switch
E2 | BRN | 9 | BCM - Park Lamp Switch
E3 | BRN | 4 | Ignition Switch
E4 | GRY/BLK | 745 | BCM
E5 | LT GRN | 24 | UHFB
E6 | BLK | 1576 | Decklid Switch
E7 | WHT | 1310 | Engine to I/P Inline
E8-E9 | -- | -- | Not Used
E10 | LT BLU | 20 | Cruise Control Module
E11 | WHT | 193 | BCM
E12 | BRN | 641 | Vehicle Speed Signal Modifier (L81) Heated Traction Switch
F1 | BLK | 550 | Ground
F2 | YEL | 43 | Radio
F3 | BRN | 4 | RIPFB
F4 | YEL | 743 | BTSI/BCM
F5 | TAN | 683 | HVAC Module
F6 | -- | -- | Not Used
F7 | BRN | 641 | HVAC Switch
F8 | PPL | 30 | Engine to I/P Inline
F9 | GRY | 8 | BCM
F10 | LT BLU | 20 | UHFB - Brake Switch
F11 | ORN | 1240 | UHFB
F12 | BRN | 641 | Traction Switch Fog Lamp Switch Heated Seat Switch

#### I/P Fuse Block - Right - Body -- Right Kick Panel

Insert Graphic SMELC80249AB2
Connector Part Information |

• | 15326717

• | Gray

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1 | BLK | 450 | Ground - Right Heated Mirror
A2 | TAN | 694 | Driver Door Unlock
A3 | -- | -- | Not Used
A4 | GRY | 295 | Right Front Door Lock - Fuel Doors
A5 | BRN | 141 | Heated Seats
A8 | ORN | 1340 | Premium Sound Amplifier
A9 | ORN | 640 | Power Seat
A10 | LT GRN | 559 | Left Heated Seat
A11 | YEL | 143 | Sunroof (Sedan) Rear Wiper (Wagon)
A12-B1 | -- | -- | Not Used
B2 | TAN | 294 | Rear Door Unlock Switch
B3 | -- | -- | Not Used
B4 | GRY | 295 | Left Front and Rear Door Lock
B5 | ORN | 267 | heated Mirrors
B8 | -- | -- | Not Used
B9 | ORN | 340 | Front Door Lock Switch
B10 | YEL | 243 | Left Window Switch
B11-B12 | -- | -- | Not Used
C1 | TAN | 683 | LIPFB
C2 | TAN | 294 | Right Front Door Unlock - Fuel Filler Door
C3 | -- | -- | Not Used
C4 | GRY | 295 | Right Front Door Lock
C5 | ORN/BLK | 780 | Door Lock Switch
C8 | BLK | 402 | Headliner
C9 | RED/BLK | 781 | Front Door Unlock Switch
C10 | YEL | 243 | Right Window Switch
C11 | PNK/BLK | 1503 | Right Heated Seat
C12 | ORN | 340 | Liftgate Inline

#### I/P Fuse Block - Right - I/P -- Right Kick Panel

Insert Graphic SMELC80214AB1
Connector Part Information |

• | 15303512

• | Gray

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1-B8 | -- | -- | Not Used
B9 | BRN | 9 | Fog Lamp Switch
B10-C1 | -- | -- | Not Used
C2 | WHT | 194 | BCM
C3-C5 | -- | -- | Not Used
C8 | PPL | 34 | UHFB
C9 | BRN | 9 | LIPFB
C10-D5 | -- | -- | Not Used
D8 | RED | 402 | UHFB
D9 | ORN/BLK | 781 | BCM
D10 | -- | -- | Not Used
D11 | BRN | 4 | LIPFB
D12-E3 | -- | -- | Not Used
E4 | RED/BLK | 780 | BCM
E5 | ORN | 300 | Ignition Switch
E6-E7 | -- | -- | Not Used
E8 | YEL | 317 | Fog Lamp Switch
E9 | -- | -- | Not Used
E10 | PNK/BLK | 1503 | Right Heated Seat Switch
E11 | YEL | 143 | UHFB
E12-F1 | -- | -- | Not Used
F2 | LT GRN | 1391 | BCM
F3 | -- | -- | Not Used
F4 | LT BLU | 195 | BCM
F5 | ORN | 300 | Ignition Switch
F6 | -- | -- | Not Used
F7 | ORN | 1440 | UHFB
F8-F9 | -- | -- | Not Used
F10 | LT GRN | 554 | Right Heated Seat Switch
F11-F12 | -- | -- | Not Used

#### Underhood Fuse Block - Engine -- Left Engine Compartment - Under UHFB

Insert Graphic SMELC80215AB1
Connector Part Information |

• | 15303513

• | Black

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1-A2 | -- | -- | Not Used
A3 | YEL | 772 | Neutral Start Safety Switch - Engine to I/P Inline
A4 | ORN | 2640 | Injector 2 (L81)
A5 | -- | -- | Not Used
A6 | PPL | 415 | Air Solenoid (L61)
PNK | 339 | EBTCM (L81)
A7 | BRN | 582 | ECM/TPS (L81)
BLK | 150 | Ground Splice (L61)
A8 | BLK | 150 | Wiper Motor
A9 | LT BLU | 20 | TCM (L81)
PNK | 839 | PCM (L61)
A10 | LT BLU | 20 | EBTCM (L81)
PNK | 139 | Injector 3 (L61)
A11 | BRN | 2192 | EBTCM (L61)
BLK | 196 | Wiper Motor (L81)
A12 | WHT | 776 | Neutral Start Safety Switch (L61) - Engine to I/P Inline
B1 | -- | -- | Not Used
B2 | ORN | 2440 | LEGR (L81)
B3 | YEL | 772 | PCM (L61) TCM (L81)
B4 | BLK/WHT | 771 | NSBU (L81)
B5 | -- | -- | Not Used
B6 | PNK | 339 | ECM (L81)
B7 | BRN | 582 | ECM (L81)
BLK | 150 | Secondary Air Pump (L61)
B8 | BLK | 150 | Heated O2 Sensor (L61)
B9 | -- | -- | Not Used
B10 | LT BLU | 20 | ECM (L81)
PNK | 139 | Injector 2 (L61)
B11 | PNK | 139 | Injector 4 (L61)
BLK/WHT | 257 | ECM (L81)
B12 | WHT | 776 | PCM (L61) TCM (L81)
C1-C3 | -- | -- | Not Used
C4 | GRN/WHT | 459 | PCM (L61) ECM (L81)
C5 | ORN | 2740 | ECM (L81)
BLK/WHT | 771 | NSBU (L61)
C6-C7 | -- | -- | Not Used
C8 | BLK | 150 | Ground Splice (L81)
C9 | PNK | 889 | Transmission (L61) TCM (L81)
C10 | LT GRN | 497 | ECM (L81)
PNK | 139 | Injector 1 (L61)
C11 | PPL | 1500 | PCM (L61)
BLK/WHT | 257 | LEGR (L81)
C12 | LT GRN | 24 | Back-Up Switch (L61 - Manual)
GRY | 773 | Neutral Start Safety Switch (L61 - Automatic) PCM (L61)
D1 | ORN | 480 | TCM (L81)
D2-D5 | -- | -- | Not Used
D8 | BLK | 150 | Coolant Flow Pump A/C Compressor Clutch (L81)
D9 | PNK | 839 | --
D10 | -- | -- | Not Used
D11 | BLK/WHT | 251 | ECM (L81)
PNK | 339 | EBTCM (L61)
D12 | YEL | 581 | ECM (L81)
GRY | 2561 | Neutral Start Safety Switch (L61 Automatic)
E1 | LT BLU | 20 | PCM (L61)
GRY | 2561 | ECM (L81)
E2 | -- | -- | Not Used
E3 | BRN | 1341 | Canister Purge (L61)
ORN | 2440 | R O2 Sensor (L81) Canister Purge (L81)
E4 | DK GRN | 59 | A/C Clutch
E5 | ORN | 2740 | ECM (L81)
BLK/WHT | 771 | PCM (L61)
E6 | BLK | 150 | A/C Compressor Switch (L61)
ORN | 2740 | ECM (L81)
E7 | ORN | 2740 | RH O2 Sensor (L81)
E8 | BLK | 150 | EBTCM (L61)
E9 | PNK | 239 | Neutral Start Safety Switch
E10 | LT GRN | 867 | EBTCM (L61)
PNK | 1539 | Ignition Coils (L81)
E11 | LT BLU | 832 | EBTCM (L61)
GRY | 773 | Ignition Coils (L81)
E12 | BLK | 196 | Wiper Motor (L61)
YEL | 581 | ECM (L81) TPS (L81)
F1 | LT BLU | 20 | EBTCM (L61)
ORN | 480 | ECM (L81)
F2 | ORN | 2440 | F O2 Sensor (L81) Mass Air Flow (L81)
BRN | 1341 | RH O2 Sensor (L61)
F3 | DK BLU | 473 | PCM (L61)
ORN | 2640 | Intake Manifold (L81)
F4 | ORN | 480 | ECM (L81)
BLK/WHT | 771 | TCM (L81)
F5 | LT GRN | 24 | Back-Up Switch (L61 Manual) Neutral Start Safety Switch (L61 Automatic)
DK BLU | 473 | ECM (L81)
F6 | BLK/WHT | 2022 | Coolant Pump (L81)
BLK/WHT | 78 | Secondary Air Pump
F7 | ORN | 2740 | FH O2 Sensor (L81)
ORN | 436 | PCM (L61)
F8 | BLK | 150 | Air Pump (L61) Redundant Ground (L81)
F9 | PPL | 1500 | Neutral Start Safety Switch (L81)
PNK | 239 | Back-Up Switch (L61)
F10 | PNK | 1639 | EIS (L61)
PNK | 1539 | Ignition Coils 1, 3, 5 (L81)
F11 | BLK | 465 | PCM (L61)
GRY | 773 | TCM (L81)
F12 | DK GRN | 35 | PCM (L61) ECM (L81)

#### Underhood Fuse Block - I/P -- Left Engine Compartment - Under UHFB

Insert Graphic SMELC80214AA1
Connector Part Information |

• | 15303512

• | Gray

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1 | DK BLU | 15 | LIPFB
A2 | WHT | 2561 | ECM (L81 Only)
A3 | BLK | 28 | BCM/Horn Switch
A4 | ORN | 2740 | LIPFB (L81 Only)
A5 | ORN | 480 | ECM (L81 Only)
A6 | PPL | 1500 | Parklock/PRNDL
A7 | BLK/WHT | 351 | ECM (L81 Only)
A8 | LT BLU | 14 | LIPFB
A9 | BRN | 741 | Cruise Switch
A10 | ORN | 540 | Stop Lamp Switch
A11 | PNK | 239 | Hazard Switch
A12 | RED | 228 | BCM/Wiper Switch
B1 | -- | -- | Not Used
B2 | PPL | 34 | RIPFB
B3 | BRN | 9 | LIPFB
B4 | ORN | 300 | LIPFB (L61 Only)
B5 | BLK | 350 | ABS Module
B6 | DK GRN | 500 | Ignition Switch
B7 | ORN | 2740 | Fuel Pump (L81 Only)
B8 | ORN | 2740 | ECM (L81 Only)
B9 | PNK | 339 | ECM (L81 Only) Cruise Control Module (L61 Only)
B10 | -- | -- | Not Used
B11 | GRY | 773 | PRNDL
B12 | LT GRN | 24 | Back-Up Lamps
C1 | -- | -- | Not Used
C2 | ORN | 1640 | BCM
C3 | WHT | 1579 | BCM
C4 | -- | -- | Not Used
C5 | BLK | 350 | ABS Module
C8 | ORN | 2740 | ECM (L81 Only)
C9 | PNK | 339 | BCM/Cruise Brake Switch
C10 | -- | -- | Not Used
C11 | ORN | 440 | LIPFB/Radio
C12 | ORN | 2140 | DLC/Radio
D1 | GRN/BLK | 592 | BCM
D2 | -- | -- | Not Used
D3 | BRN | 1341 | LIPFB/Cruise Clutch Switch
D4 | ORN | 1440 | RIPFB
D5 | BLK | 350 | ABS Splice Pack
D8 | ORN | 240 | Headlamp/Turn Signal Switch
D9 | -- | -- | Not Used
D10 | PNK | 9 | SDM/PRNDL
D11 | -- | -- | Not Used
D12 | DK BLU | 473 | ECM (L81 Only)
E1 | ORN | 2240 | Cigar Lighter
E2 | -- | -- | Not Used
E3 | PNK | 39 | Cluster/Coolant Sensor
E4 | ORN | 1740 | Auxiliary Power Outlet
E5 | -- | -- | Not Used
E6 | DK GRN | 392 | BCM/Wiper Switch
E7 | ORN | 1240 | LIPFB
E8 | PNK | 1200 | Headlamp Switch
E9 | PNK | 3 | Ignition Switch
E10 | ORN | 1040 | Hazard Switch
E11 | ORN | 2540 | BCM
E12-F1 | -- | -- | Not Used
F2 | PNK | 1200 | BCM/Low Beam Headlamp Switch
F3 | DK GRN | 335 | ECM (L81 Only)
F4 | -- | -- | Not Used
F5 | ORN | 1140 | Fuel Pump Relay
F6 | BLK/WHT | 99 | BCM
F7 | -- | -- | Not Used
F8 | PNK | 1200 | BCM/Fog Lamp Switch
F9 | BLK/WHT | 771 | PRNDL
F10-F11 | -- | -- | Not Used
F12 | ORN | 2540 | Decklid Release/Cluster

#### Underhood Fuse Block - Forward Lamp -- Left Engine Compartment - Under UHFB

Insert Graphic SMELC86785AA1
Connector Part Information |

• | 15328719

• | Dark Gray

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1 | ORN | 140 | Low Beam - Right
A2 | -- | -- | Not Used
A3 | DK BLU | 473 | Fan Control Module (L61)
DK BLU | 1201 | Low Beam Left
A4 | -- | -- | Not Used
A5 | DK BLU | 473 | Fan Control Module (L81)
A6 | BLK | 2022 | Fan Control Module (L81)
A7 | -- | -- | Not Used
A8 | PNK | 839 | Fan Control Module
A9-A10 | -- | -- | Not Used
A11 | BLK | 150 | Left Forward Lamp Ground Splice Pack
A12 | DK GRN | 335 | Cooling Fan
B1 | DK BLU | 593 | High Beam - Right
B2-B8 | -- | -- | Not Used
B9 | BRN | 9 | Park Lamp - Right
B10-B12 | -- | -- | Not Used
C1 | BLK/WHT | 99 | Low Washer Fluid (L61)
LT BLU | 14 | Turn - Left (L81)
C2 | -- | -- | Not Used
C3 | DK BLU | 1201 | Low Beam - Right (L81)
C4-C8 | -- | -- | Not Used
C9 | BRN | 9 | Park Lamp - Left
C10-C12 | -- | -- | Not Used
D1 | ORN | 40 | High Beam - Left
D2-D3 | -- | -- | Not Used
D4 | DK GRN | 29 | Horn
D5 | -- | -- | Not Used
D8 | RED | 228 | Washer Pump (L61)
D9 | BRN | 9 | Side Marker Lamp - Right
D10-D12 | -- | -- | Not Used
E1 | ORN | 40 | Low Beam - Left
E2 | -- | -- | Not Used
E3 | DK BLU | 1201 | Low Beam - Left (L61)
PNK | 1200 | High Beam - Left (L81)
E4 | -- | -- | Not Used
E5 | PPL | 34 | Fog Lamp - Right
E6 | DK GRN | 392 | Washer Pump (L81)
E7-E8 | -- | -- | Not Used
E9 | BRN | 9 | Side Marker Lamp - Left
E10 | PNK | 1200 | High Beam - Left (L61)
E11-E12 | -- | -- | Not Used
F1 | DK BLU | 15 | Turn - Right
F2 | -- | -- | Not Used
F3 | DK BLU | 1201 | Low Beam - Right (L61)
PNK | 1200 | High Beam - Right (L81)
F4 | -- | -- | Not Used
F5 | PPL | 34 | Fog Lamp - Left
F6 | BLK/WHT | 99 | Low Washer Fluid (L81)
F7 | -- | -- | Not Used
F8 | LT BLU | 14 | Turn - Left (L61)
RED | 228 | Washer Pump (L81)
F9 | DK GRN | 392 | Washer Pump (L61)
F10 | PNK | 1200 | High Beam - Right (L61)
F11-F12 | -- | -- | Not Used