For 1990-2009 cars

### Removal Procedure

1. Operate the sunroof to the open position.
2. Remove the plastic clips (2) from the rear of the deflector on each side using the needle pliers.
3. Use the pliers to squeeze the tangs of the clips together under the wind deflector to release.

### Installation Procedure

1. Use the pliers to squeeze the tangs of the clips together under the wind deflector to install.
2. Install the plastic clips (2) to the rear of the deflector on each side using the needle pliers.
3. Ensure the rear clips are in the 2 holes on each side of the U-channel.
4. Verify smooth operation of the sunroof in all positions.