For 1990-2009 cars

### Removal Procedure

1. Unsnap the sunshade from the sunshade inner retainer clip. Move the sunshade to the side.
2. Remove the sunshade retainer fastener and retainer.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the sunshade retainer with the retainer fastener.

Tighten
Tighten 7the inner sunshade support fasteners to 15 N·m (11 lb ft).

2. Snap the sunshade back into the retainer.