For 1990-2009 cars

# SMU and Quick Reference Specifications Guide Update for 2001 and 2002 L Series (L61) Engine Regarding Incorrect Cylinder Head Bolt Torque Specifications

Subject: | Service Manual and Quick Reference Specifications Guide Update for 2001 and 2002 L-Series (L61) Engine Regarding Incorrect Cylinder Head Bolt Torque Specifications

Models: | 2001-2002 Saturn L-Series Vehicles

### Purpose

The purpose of this bulletin is to update all 2001 and 2002 L-Series (L61) Engine Service Manuals and 2001-2002 L-Series Quick Reference Specifications Guide at your location.

Please obtain all of the 2001 and 2002 L-Series (L61) Engine Service Manuals and 2001-2002 L-Series Quick Reference Specifications Guide and make the necessary corrections as indicated below.

1. 2001 L-Series (L61) Engine Service Manual

• | Page 19. Cross out the + 185° reference.

• | Page 561. Cross out the + 185° reference.

2. 2002 L-Series (L61) Engine Service Manuals

Page 570. Cross out the + 185° reference.

3. 2001-2002 L-Series Quick Reference Specifications Guide

• | 2001 (L61) - Page 250. Cross out the + 185° reference.

• | 2002 (L61) - Page 255. Refer to procedure in the "Mechanical" section of the L61 Engine Service Manual (page 570).

After the corrections have been made, the torque specification should read as follows:

Tighten
Tighten the Cylinder Head Bolts to 30 N·m (22 lb ft) + 155°