For 1990-2009 cars

Table 1: | Switch Inputs
Table 2: | Exterior Lamps
Table 3: | Interior Lamps
Table 4: | Door Locks
Table 5: | Security Data

The following tables lists the data directly related to the RKE/security system only.

#### Switch Inputs

Scan Tool Output Control | Description
--- | ---
Battery 1 | Volts
Driver Door Switch | High/Low
Pass Door Switches | High/Low
Decklid Ajar Switch | High/Low
High Beam Input = OFF | Yes/No
High Beam Input = DRL | Yes/No

#### Exterior Lamps

Scan Tool Output Control | Description
--- | ---
Battery 1 | Volts
High Beam Input | Volts
High Beam Input = OFF | Yes/No
High Beam Input = DRL | Yes/No
High Beam Input = High | Yes/No
DRL Relay Command | On/Off
DRL Relay Feedback | High/Low

#### Interior Lamps

Scan Tool Output Control | Description
--- | ---
Battery 1 | Volts
Dome Lamp Command | On/Off
Dome Lamp Feedback | High/Low

#### Door Locks

Scan Tool Output Control | Description
--- | ---
Battery 1 | Volts
Driver Unlock Relay Command | On/Off
Driver Unlock Relay Feedback | High/Low
Pass Unlock Relay Command | On/Off
Pass Unlock Relay Feedback | High/Low
Lock All Relay Command | On/Off
Lock All Relay Feedback | High/Low
Remote Lock Command | Yes/No
Remote Unlock Command | Yes/No
Remote Panic Command | Yes/No
Remote Trunk Command | Yes/No
Remote Programmed | Yes/No
Trunk Release Solenoid Command | On/Off
Trunk Release Solenoid Feedback | High/Low

#### Security Data

Scan Tool Output Control | Description
--- | ---
Battery 1 | Volts
Ignition 1 Input | High/Low
Accessory | High/Low
Horn Relay Command | On/Off
Horn Relay Feedback | High/Low
Decklid Ajar Switch | High/Low
Trunk Release Switch | On/Off