For 1990-2009 cars

### Removal Procedure

1. Disengage park brake boot by squeezing at attachment locations.
2. Lift boot out of the way.
3. Pull up firmly on cup holder to disengage cup holder from console.
4. Remove cup holder.

### Installation Procedure

1. Position cup holder to console and push firmly at snap locations to engage cup holder to console.
2. Position park brake boot to console and push firmly at attaching locations to engage park brake boot to console.