For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Amplifier to I/P Beam Fasteners | 10 N·m | 89 lb in
Antenna Base to Roof Panel Nut -- Wagon | 6 N·m | 53 lb in
Antenna Bracket to Rear Fender Fasteners -- Sedan | 8 N·m | 71 lb in
Antenna Mast to Antenna Base | 8 N·m | 71 lb in
CD Changer/Player Bracket to Vehicle Fastener -- Sedan | 8 N·m | 71 lb in
CD Changer/Player Compartment to Vehicle Fasteners -- Wagon | 8 N·m | 71 lb in
CD Changer/Player to CD Changer/Player Bracket Fasteners -- Sedan | 4 N·m | 35 lb in
CD Changer/Player to CD Changer/Player Compartment Fasteners | 4 N·m | 35 lb in
Cargo Net Fasteners | 2.5 N·m | 22 lb in
Glove Compartment Bin to I/P Fasteners | 2.5 N·m | 22 lb in
Glove Compartment Door Fasteners | 2 N·m | 18 lb in
Radio Ground Strap to H-Brace Stud Fasteners | 6 N·m | 53 lb in
Radio to I/P Fasteners | 2.5 N·m | 22 lb in
Subwoofer Speaker to Rear Shelf Attaching Fasteners -- Sedan | 2.5 N·m | 22 lb in
Subwoofer Speaker to Vehicle Attaching Fasteners -- Wagon | 5 N·m | 44 lb in
Woofer Speaker to Door Attaching Fasteners | 1.5 N·m | 13 lb in