For 1990-2009 cars

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Key On, Engine Off
Battery 1 | BCM Data | Volts | 9 to 16 volts
Decoded Switch State | BCM Data | Undecided, Lock, Unlock, Off | Off
Door Lock Switch | BCM Data | Volts | 13 volts
Driver Door Switch | BCM Data | open/closed | closed
Driver Door Unlock Fdbk. | BCM Data | ON/OFF | OFF
Fob ID | BCM Data | None, Fob 1, Fob 2, Fob 3, Fob 4 | Fob 1
Lock All Doors Fdbk. | BCM Data | ON/OFF | ON
Pass Door Switch | BCM Data | open/closed | closed
RKE Low Battery | BCM Data | Yes/No | NO
RKE Sinc | BCM Data | Yes/No | YES
RKE Lock Button | BCM Data | ON/OFF | OFF
RKE Unlock Button | BCM Data | ON/OFF | OFF
RKE Trunk Button | BCM Data | ON/OFF | OFF
RKE Panic Button | BCM Data | ON/OFF | OFF
Trunk Release | BCM Data | ON/OFF | OFF
Unlock All Doors Fdbk. | BCM Data | ON/OFF | ON