For 1990-2009 cars

### Removal Procedure

1. Operate the sunroof to the open position.
2. Use needle pliers to emove the plastic clips from the rear of the air deflector on each side.
3. Use pliers to squeeze the tabs of the clips together under the air deflector to release.
4. Remove the air deflector from the sunroof.

### Installation Procedure

1. Position the air deflector from the sunroof.
2. Install the air deflector. Use pliers to squeeze the tabs of the clips together under the air deflector.
3. Use needle pliers to install the plastic clips to the rear of the deflector on each side.
4. Ensure the rear clips are in the 2 holes on each side of the U-channel.
5. Inspect the operation of the sunroof in all positions.