For 1990-2009 cars

#### Audio Amplifier C1

Connector Part Information |

• | 15336186

• | 15-Way F (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | BN | 199 | Left Rear Speaker Output (+)
2 | BU | 46 | Right Rear Speaker Output (+)
3-5 | -- | -- | Not Used
6 | TN | 201 | Left Front Speaker Output (+)
7 | GN | 200 | Right Front Speaker Output (+)
8 | YE | 116 | Left Rear Speaker Output (-)
9 | BU | 115 | Right Rear Speaker Output (-)
10 | OG | 360 | Amplifier Control
11-12 | -- | -- | Not Used
13 | OG | 1950 | Amplifier Present Signal
14 | GY | 118 | Left Front Speaker Output (-)
15 | GN | 117 | Right Front Speaker Output (-)

#### Audio Amplifier C2

Connector Part Information |

• | 15336184

• | 10-Way F (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | GN | 200 | Right Front Speaker Output (+)
2 | TN | 201 | Left Front Speaker Output (+)
3 | BU | 46 | Right Rear Speaker Output (+)
4 | BN | 199 | Left Rear Speaker Output (+)
5 | GN | 117 | Right Front Speaker Output (-)
6 | GY | 118 | Left Front Speaker Output (-)
7 | BK | 450 | Ground
8 | BK | 450 | Ground
9 | BU | 115 | Right Rear Speaker Output (-)
10 | YE | 116 | Left Rear Speaker Output (-)

#### Audio Amplifier C3

Connector Part Information |

• | 15336191

• | 6-Way F (WH)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | BU | 346 | Left or Rear Subwoofer Speaker Output (+)
2 | -- | -- | Not Used
3 | GN | 1794 | [Left or Rear] Subwoofer Speaker Output (-)
4 | OG | 1340 | Battery Positive Voltage
5 | OG | 1340 | Battery Positive Voltage
6 | -- | -- | Not Used

#### Radio C1 (w/ U67)

Connector Part Information |

• | 12110088

• | 24- Way F Micro-Pack 100 Series (GY)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1-A2 | -- | -- | Not Used
A3 | OG | 360 | Amplifier Control
A4-A7 | -- | -- | Not Used
A8 | BN | 199 | Left Rear Speaker Output (+)
A9 | YE | 116 | Left Rear Speaker Output (-)
A10 | GN | 117 | Right Front Speaker Output (-)
A11 | GN | 200 | Right Front Speaker Output (+)
A12 | BK | 550 | Ground
B1 | OG | 440 | Battery Positive Voltage
B2 | YE | 43 | Accessory Voltage
B3 | OG | 2140 | Battery Positive Voltage
B4 | GY | 8 | Instrument Panel Lamp Supply Voltage
B5 | -- | -- | Not Used
B6 | OG | 1950 | Amplifier Present Signal
B7 | -- | -- | Not Used
B8 | TN | 201 | Left Front Speaker Output (+)
B9 | GY | 118 | Left Front Speaker Output (-)
B10 | BU | 115 | Right Rear Speaker Output (-)
B11 | BU | 46 | Right Rear Speaker Output (+)
B12 | BN | 9 | Park Lamp Supply Voltage

#### Radio C1 (w/o U67)

Connector Part Information |

• | 12110088

• | 24-Way F Micro-Pack Series (GY)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1-A7 | -- | -- | Not Used
A8 | BN | 199 | Left Rear Speaker Output (+)
A9 | YE | 116 | Left Rear Speaker Output (-)
A10 | D-GN | 117 | Right Front Speaker Output (-)
A11 | L-GN | 200 | Right Front Speaker Output (+)
A12 | BK | 550 | Ground
B1 | OG | 440 | Battery Positive Voltage
B2 | YE | 43 | Accessory Voltage
B3 | OG | 2140 | Battery Positive Voltage
B4 | GY | 8 | Instrument Panel Lamp Supply Voltage
B5-B7 | -- | -- | Not Used
B8 | TN | 201 | Left Front Speaker Output (+)
B9 | GY | 118 | Left Front Speaker Output (-)
B10 | L-BU | 115 | Right Rear Speaker Output (-)
B11 | D-BU | 46 | Right Rear Speaker Output (+)
B12 | BN | 9 | Park Lamp Supply Voltage

#### Radio C2

Connector Part Information |

• | 12064799

• | 12-Way F Micro-Pack 100 Series (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A-G | -- | -- | Not Used
H | DK GRN/WHT | 368 | Right Audio Signal (+)
J | BRN/WHT | 367 | Left Audio Signal (+)
K | BLK/WHT | 372 | Audio Common
L | -- | -- | Not Used
M | DK BLU | 693 | Cellular Telephone Mute Signal

#### Speaker- LF (Tweeter)

Connector Part Information |

• | 15305566

• | 2-Way F (NA)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | GY | 118 | Left Front Speaker Output (-)
2 | TN | 201 | Left Front Speaker Output (+)

#### Speaker- LF (Woofer)

Connector Part Information |

• | 12186719

• | 2-Way F (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | GY | 118 | Left Front Speaker Output (-)
2 | TN | 201 | Left Front Speaker Output (+)

#### Speaker- LR

Connector Part Information |

• | 12186719

• | Black

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | YE | 116 | Left Rear Speaker Output (-)
2 | WH | 199 | Left Rear Speaker Output (+)

#### Speaker- RF (Tweeter)

Connector Part Information |

• | 15305566

• | 2-Way F (NA)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | D-GN | 117 | Right Front Speaker Output (-)
2 | L-GN | 200 | Right Front Speaker Output (+)

#### Speaker- RF (Woofer)

Connector Part Information |

• | 12186719

• | Black

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | D-GN | 117 | Right Front Speaker Output (-)
2 | L-GN | 200 | Right Front Speaker Output (+)

#### Speaker- RR

Connector Part Information |

• | 12186719

• | Black

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | L-BU | 115 | Right Rear Speaker Output (-)
2 | D-BU | 46 | Right Rear Speaker Output (+)

#### Speaker- Subwoofer

Connector Part Information |

• | 12052832

• | 2-Way F (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | D-BU/WH | 346 | Subwoofer Speaker Output (+)
B | L-GN/BK | 1794 | Subwoofer Speaker Output (-)