For 1990-2009 cars

### Removal Procedure

1. Remove the mounting screws from the DVD player.
2. Slide the DVD player forward.
3. Disconnect the electrical connectors from the DVD player.

### Installation Procedure

1. Connect the electrical connectors to the DVD player.

Notice: Refer to Fastener Notice in the Preface section.

2. Slide the DVD player inward and fasten with screws.

Tighten
Tighten the screws to 2 N·m (18 lb in).