For 1990-2009 cars

#### Engine Oil Pressure (EOP) Switch (2.2L)

Connector Part Information |

• | 12065299

• | 4-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | TN/BK | 231 | Oil Pressure Switch Signal
2-4 | -- | -- | Not Used

#### Engine Oil Pressure (EOP) Switch (3.0L)

Connector Part Information |

• | 12176800

• | 1-Way F Metri-Pack 150 Series Sealed (GY)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | TN/BK | 231 | OIl Pressure Switch Signal

#### Instrument Panel Cluster (IPC)

Connector Part Information |

• | 15305356

• | 16-Way F Micro-Pack Series (GY)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A1 | PK | 39 | Ignition 1 Voltage
A2 | D-GN | 264 | Security Indicator Supply Voltage
A3 | -- | -- | Not Used
A4 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
A5 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
A6 | BK | 550 | Ground
A7 | -- | -- | Not Used
A8 | GY | 8 | Instrument Panel Lamp Supply Voltage
B1 | -- | -- | Not Used
B2 | OG | 2540 | Battery Positive Voltage
B3 | -- | -- | Not Used
B4 | BK | 350 | Ground
B5 | PU | 1807 | Class 2 Serial Data
B6 | PU | 1807 | Class 2 Serial Data
B7-B8 | -- | -- | Not Used