For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the General Description and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Suspension General Diagnosis
2 | Verify the vehicle leans or sways in corners. Does the vehicle operate normally? | System OK | Go to Step 3
3 | Inspect the following components for wear or damage:

• | The front springs

• | The rear springs

Are the components worn or damaged?

Go to Step 5

Go to Step 4

4 | Inspect the stabilizer shaft link for wear or damage. Is the stabilizer shaft link worn or damaged? | Go to Step 6 | Go to Step 2
5 | Replace the springs. Refer to the appropriate procedure:

• | Strut, Strut Component, and Spring Replacement in Front Suspension.

• | Shock Absorber Replacement in Rear Suspension.

Did you complete the repair?

Go to Step 7

--

6 | Replace the stabilizer shaft link. Refer to Stabilizer Shaft Link Replacement in Front Suspension. Did you complete the repair? | Go to Step 7 | --
7 | Operate the vehicle in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3