For 1990-2009 cars

Application | Fluid/Lubricant
--- | ---
Automatic Transmission Fluid | Saturn T-IV Fluid P/N 22689186.
Door Hinges, Hood, Rear Folding Seat and Liftgate Hinges | Lubricate with SAE 5W-30 engine oil. Do Not Use Aerosols.
Door Hold-Open Check Links | Lubricant with Lubriplate® grease aerosol into the case; grease top, bottom, and sides. Wipe off excess lubricant. Use Lubriplate® 70 or equivalent to lubricate Saturn P/N 21038914.
Engine Coolant | 50/50 Mixture of clean, drinkable water and use DEX-COOL® coolant, Saturn P/N 21031164.
Engine Oil | Engine oil with the American Petroleum Institute Certified for Gasoline Engines "Starburst" symbol of the proper viscosity
Five-Speed Automatic Transaxle | T-IV Fluid P/N 22689186.
Glove Box Latch | Lubricate, if necessary, with any silicone base lubricating fluid. Do Not Use Aerosols.
Hood Latch Assembly Pivots and Springs Anchor | Lubricate with SAE 5W-30 engine oil. Do Not Use Aerosols.
Hood Latch Assembly Release Pawl | Lubricate with chassis grease meeting requirements of NLGI Grade 2, Category LB GM P/N 1052497 or equivalent.
Hood, Trunk and Door Hinges | Multi-Purpose Lubricant, Superlube GM P/N 12346241 (Canadian P/N 1095474
Hydraulic Brake System | Delco Supreme 11® Brake Fluid or DOT 3 Brake Fluid, Saturn P/N 21013073.
Hydraulic Clutch System | Delco Supreme 11® Brake Fluid or DOT 3 Brake Fluid, Saturn P/N 21013073.
Key Lock Cylinders | Multi-Purpose Lubricant, Superlube GM P/N 12346241 (Canadian P/N 1095474
Manual Transmission | DEXRON® III Automatic Transmission Fluid
Parking Brake Cable Guides | Chassis Lubricant GM P/N 12377985 or equivalent or Lubricant meeting requirements of NLGI #2, Category LB or GC-LB.
Rear Drive Module and Power Transfer Unit | All-Wheel Drive Fluid, VERSATRAK® GM P/N 12378514.
Sunroof Track | Use Lubriplate® Saturn P/N 21038869 (Canadian P/N 992723) or lubricant meeting requirements of NLGI #2, Category LB or GC-LB
VTi Variable Transaxle | DEX-CVT® Fluid, P/N 22688912.
Weatherstrip COnditioning | Dielectric Silicone Grease GM P/N 12345579 (Canadian P/N 992887) or equivalent.
Windshield Washer Solvent | Add washer solvent, Saturn P/N 11051515 or equivalent, as necessary, mixed per the manufacture instructions.