For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Control Valve Body Assembly to Transmission Case | 12 N·m | 108 lb in
Manual Shift Shaft Detent Spring to Control Valve Body Assembly | 12 N·m | 108 lb in
Flange/Yoke to Output Shaft | 123 N·m | 91 lb ft
Transmission Oil Pump Cover Assembly to Torque Converter Housing | 56 N·m | 42 lb ft
Input Speed Sensor to Torque Converter Housing | 12 N·m | 108 lb in
Oil Pump Assembly to Transmission Oil Pump Cover Assembly | 26 N·m | 20 lb ft
Park/Neutral Position Switch to Transmission Case | 28 N·m | 22 lb ft
Oil Pan to Transmission Case | 26 N·m | 20 lb ft
Output Speed Sensor to Low and Reverse Clutch Piston Housing | 12 N·m | 108 lb in
Transmission Fluid Pressure Switch to Main Valve Body Assembly | 12 N·m | 108 lb in
Power Take-Off (PTO) Cover to Transmission Case | 43 N·m | 32 lb ft
Low and Reverse Clutch Piston Housing to Transmission Case | 56 N·m | 42 lb ft
Manual Shift Shaft Nut | 24 N·m | 17 lb ft
Shift Valve Body to Main Valve Body | 12 N·m | 108 lb in
Shipping Bracket to Torque Converter Assembly | 27 N·m | 20 lb ft
Turbine Speed Sensor to Transmission Case | 12 N·m | 108 lb in