For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Power Window Schematics Connector End View Reference: Power Door Systems Connector End Views
1 | Did you perform the Door Systems Diagnostic System Check? | Go to Step 2 | Go to Diagnostic System Check - Door Systems
2 | Operate the driver window. Does the window operate normally with the exception of the express down function? | Go to Step 3 | Go to Symptoms - Doors
3 | Replace the driver power window switch. Refer to Front Side Door Window Switch Replacement . Is the repair complete? | Go to Step 4 | --
4 | Operate the system to verify the repair. Did you correct the condition? | System OK | --