For 1990-2009 cars

Table 1: | Crankshaft Position (CKP) Sensor
Table 2: | Engine Coolant Temperature (ECT) Sensor
Table 3: | Engine Oil Pressure (EOP) Switch
Table 4: | Evaporative Emission (EVAP) Canister Purge Solenoid
Table 5: | Evaporative Emission (EVAP) Canister Vent Solenoid
Table 6: | Fuel Injector 1
Table 7: | Fuel Injector 2
Table 8: | Fuel Injector 3
Table 9: | Fuel Injector 4
Table 10: | Fuel Pump and Sender Assembly
Table 11: | Fuel Tank Pressure (FTP) Sensor
Table 12: | Heated Oxygen Sensor (HO2S)- Front
Table 13: | Heated Oxygen Sensor (HO2S)- Rear
Table 14: | Idle Air Control (IAC) Valve
Table 15: | Ignition Control Module (ICM)
Table 16: | Intake Air Temperature (IAT) Sensor
Table 17: | Knock Sensor (KS)
Table 18: | Manifold Absolute Pressure (MAP) Sensor
Table 19: | Secondary Air Injection (AIR) Solenoid
Table 20: | Secondary Air Injection (AIR) Pump
Table 21: | Throttle Position (TP) Sensor

#### Crankshaft Position (CKP) Sensor

Connector Part Information |

• | 12162193

• | 2-Way F Metri-Pack 150.2 Series Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PU | 574 | Low Reference
B | YE | 573 | CKP Sensor Signal

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information |

• | 12162195

• | 2-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | BK | 2761 | Low Reference
B | YE | 410 | ECT Sensor Signal

#### Engine Oil Pressure (EOP) Switch

Connector Part Information |

• | 12065299

• | 4-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | TN/BK | 231 | Oil Pressure Switch Signal

#### Evaporative Emission (EVAP) Canister Purge Solenoid

Connector Part Information |

• | 12052643

• | 2-Way F Metri-Pack 150 Series Sealed (RD)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PK | 139 | Ignition 1 Voltage
B | D-GN/WH | 428 | EVAP Canister Purge Solenoid Control

#### Evaporative Emission (EVAP) Canister Vent Solenoid

Connector Part Information |

• | 12052643

• | 2-Way F Metri-Pack 150 Series Sealed (RD)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | OG | 2740 | Ignition 1 Voltage
B | WH | 1310 | EVAP Canister Vent Solenoid Control

#### Fuel Injector 1

Connector Part Information |

• | 15236181

• | 2-Way F (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PK | 139 | Ignition 1 Voltage
B | BK | 1744 | Fuel Injector 1 Control

#### Fuel Injector 2

Connector Part Information |

• | 15236181

• | 2-Way F (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PK | 139 | Ignition 1 Voltage
B | L-GN/BK | 1745 | Fuel Injector 2 Control

#### Fuel Injector 3

Connector Part Information |

• | 15236181

• | 2-Way F (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PK | 139 | Ignition 1 Voltage
B | PK/BK | 1746 | Fuel Injector 3 Control

#### Fuel Injector 4

Connector Part Information |

• | 15236181

• | 2-Way F (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PK | 139 | Ignition 1 Voltage
B | L-BU/BK | 844 | Fuel Injector 4 Control

#### Fuel Pump and Sender Assembly

Connector Part Information |

• | 15326631

• | 4-Way F GT 280 Sealed 5.8 (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PU | 30 | Fuel Level Sensor Signal
B | GY | 120 | Fuel Pump Supply Voltage
C | BK | 650 | Ground
D | BK | 2759 | Low Reference

#### Fuel Tank Pressure (FTP) Sensor

Connector Part Information |

• | 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
1 | GY | 2709 | 5 Volt Reference
2 | BK | 2759 | Low Reference
3 | D-GN | 890 | Fuel Tank Pressure Sensor Signal

#### Heated Oxygen Sensor (HO2S)- Front

Connector Part Information |

• | 12160482

• | 4-Way F (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | TN | 1667 | HO2S Low Signal
B | PU | 1666 | HO2S High Signal
C | D-GN | 676 | HO2S Heater Low Control
D | PK | 1639 | Ignition 1 Voltage

#### Heated Oxygen Sensor (HO2S)- Rear

Connector Part Information |

• | 12160825

• | 4-Way M Metri-Pack 150 Series (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | TN/WH | 1669 | HO2S Low Signal
B | PU/WH | 1668 | HO2S High Signal
C | BK/WH | 1423 | HO2S Heater Low Control
D | PK | 1639 | Ignition 1 Voltage

#### Idle Air Control (IAC) Valve

Connector Part Information |

• | 15354716

• | 4-Way F GT150 Series Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | L-GN/BK | 444 | IAC Coil B High Control
B | L-GN/WH | 1749 | IAC Coil B Low Control
C | L-BU/BK | 1748 | IAC Coil A Low Control
D | L-BU/WH | 1747 | IAC Coil A High Control

#### Ignition Control Module (ICM)

Connector Part Information |

• | 15329032

• | 9-Way F (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PK | 1639 | Ignition 1 Voltage
B | WH | 423 | IC Timing Control
C-D | -- | -- | Not Used
E | BK | 250 | Ground
F | BN/WH | 633 | Camshaft Position Signal
G | OG | 406 | IC Timing Control B

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | 12162199

• | 2-Way F GT 150 Sealed 3.2x4.0 (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | GY | 720 | Low Reference
B | TN | 472 | IAT Sensor Signal

#### Knock Sensor (KS)

Connector Part Information |

• | 12077900

• | 2-Way F Metri-Pack 280 Series Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | D-BU | 496 | Knock Sensor Signal
B | GY | 1716 | Low Reference

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | 12129946

• | 3-Way F Metri-Pack 150 Series Sealed (M GY)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | GY | 2704 | 5 Volt Reference
B | OG/BK | 469 | Low Reference
C | L-GN | 432 | MAP Sensor Signal

#### Secondary Air Injection (AIR) Solenoid

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PK/BK | 415 | AIR Solenoid Supply Voltage
B | PK/BK | 429 | AIR Solenoid Control

#### Secondary Air Injection (AIR) Pump

Connector Part Information |

• | 12191968

• | 2-Way F Metri-Pack 280 Series Sealed (L-GY)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | RD | 78 | AIR Pump Supply Voltage
B | BK | 150 | Ground

#### Throttle Position (TP) Sensor

Connector Part Information |

• | 12110192

• | 3-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | GN | 2701 | 5 Volt Reference
B | BK | 2752 | Low Reference
C | D-BU | 417 | TP Sensor Signal