For 1990-2009 cars

### Removal Procedure

1. Lift the rear wiper arm away from the window.
2. Remove the existing wiper blade insert by pulling downward at the wiper blade end to disengage the retaining tab.

Pull the blade insert out of the wiper blade.

### Installation Procedure

1. Install the wiper blade insert by sliding it through the wiper blade claws until fully seated and the wiper arm tab is seated into the wiper blade insert.
2. Reposition the rear wiper arm to the window.