For 1990-2009 cars

1. Remove the manual shaft to transmission case pin (803).

Important: The parking lock actuator assembly (807) remains attached to the manual shaft and detent lever until the assembly is removed.

2. Remove the manual shaft and detent lever assembly (806) by pushing the manual shaft into the transmission case (51). The parking lock actuator assembly (807) remains attached to the detent lever until you remove the manual shaft and detent lever assembly.

Notice: Do not damage the case bore during removal of the manual shift shaft seal.

3. Remove the manual shaft seal (809) from the case (51).