For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Assist Handle Bracket to Roof Rail | 16 N·m | 12 lb ft
Assist Handle Fasteners | 16 N·m | 12 lb ft
Cargo Net Fasteners | 2.5 N·m | 22 lb in
Child Seat Tether Bracket Fasteners | 20 N·m | 15 lb ft
Console Fasteners | 2.5 N·m | 22 lb in
Curtain Inflator Retaining Bolt (10 mm Hex Head) | 10 N·m | 89 lb in
Door Inner Pull Handle Fasteners | 1.5 N·m | 13 lb in
Door Trim Panel Fasteners | 1.5 N·m | 13 lb in
Inner Sunshade Support Fasteners | 15 N·m | 11 lb ft
Liftgate Inner Pull Handle Fasteners | 5 N·m | 44 lb in
Rear Shoulder Belt Upper Fasteners | 35 N·m | 26 lb ft
Seat Attachment Bolts | 25 N·m | 19 lb ft
Shoulder Belt Height Adjuster Fasteners | 35 N·m | 26 lb ft
Shoulder Belt to Seat Frame Bolt | 35 N·m | 26 lb ft
Sunshade to Headliner Fasteners | 15 N·m | 11 lb ft
Upper Molding Fastener | 5 N·m | 44 lb in
Windshield Pillar Trim | 5 N·m | 44 lb in