For 1990-2009 cars

### Removal Procedure

1. Remove the wiper arms. Refer to Windshield Wiper Arm Replacement in Wipers/Washer Systems.
2. Remove the rear hood seal. Refer to Hood Rear Seal Replacement .
3. Remove the air inlet grille from the vehicle.

### Installation Procedure

1. Install the air inlet grille to the vehicle.
2. Install the rear hood seal. Refer to Hood Rear Seal Replacement .
3. Install the wiper arms. Refer to Windshield Wiper Arm Replacement in Wipers/Washer Systems.