For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Frame Mounting Bolts

- First Pass

90 N·m

66 lb ft

- Second Pass

+45°-60°

O2 Sensor Clamp Nut | 4 N·m | 35 lb in
Splash Shield Body Bolts | 5 N·m | 45 lb in
Steering Gear Bolts | 60 N·m | 44 lb ft
Suspension Support Bolts

- First Pass

90 N·m

66 lb ft

- Second Pass

+45°-60°

Transmission Mount Through Bolt - Front | 55 N·m | 41 lb ft
Transmission Mount Through Bolt - Rear | 90 N·m | 66 lb ft