For 1990-2009 cars

### Removal Procedure

1. Remove the headliner. Refer to Headlining Trim Panel Replacement in Interior Trim.
2. Remove the corner upper garnish molding . Refer to Body Rear Corner Upper Garnish Molding Replacement in Interior Trim.
3. Remove the rear trunk trim. Refer to Rear Compartment Closeout Panel Replacement in Interior Trim.
4. Remove the antenna cable (2) from the module (1).
5. Remove the antenna cable (2) from the vehicle.

### Installation Procedure

1. Install the antenna cable (2) to the vehicle.
2. Install the antenna cable (2) to the module (1).
3. Install the rear trunk trim. Refer to Rear Compartment Closeout Panel Replacement in Interior Trim.
4. Install the corner upper garnish molding . Refer to Body Rear Corner Upper Garnish Molding Replacement in Interior Trim.
5. Install the headliner. Refer to Headlining Trim Panel Replacement in Interior Trim.