For 1990-2009 cars

#### Left Heated Seat/Fog Lamp Switch

Connector Part Information |

• | 12186098

• | 8-Way F Metri-Pack 150 Series (L-GY)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | PK | 1200 | Headlamp High Beam Ground
B | BN | 9 | Park Lamp Supply Voltage
C | YE | 317 | Fog Lamp Relay Control Circuit
D | GY | 8 | Instrument Panel Lamp Supply Voltage
E | BK | 550 | Ground
F | PK | 1501 | Driver Heated Seat High/Low Signal
G | YE | 182 | Heated Seat Control Module Inhibit Signal
H | BN | 641 | Ignition 3 Voltage

#### Right Heated Seat/Traction Switch

Connector Part Information |

• | 12047886

• | 8-Way F Metri-Pack Series (BK)

Pin | Wire Color | Circuit Number | Function
--- | --- | --- | ---
A | BN | 641 | Ignition 3 Voltage
B | D-BU | 1660 | Traction Control Indicator Control
C | L-BU | 1788 | Traction Control Switch Signal
D | GY | 8 | Instrument Panel Lamp Supply Voltage
E | BK | 550 | Ground
F | PK/BK | 1503 | Passenger Heated Seat High/Low Signal
G | L-GN | 559 | Passenger Heated Seat On Signal
H | -- | -- | Not Used