For 1990-2009 cars

#### Body Control Module

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Door Lock Test | Driver Door Unlock | The BCM actuates the driver door unlock relay when you select ON. Driver door should unlock.
Door Lock Test | All Doors Lock | The BCM actuates the door lock relay when you select ON. All doors should lock.
Door Lock Test | Passenger Door Unlock | The BCM acuates the door unlock relay and the driver door unlock relay when you select ON. All doors should unlock.